void setup() {

// put your setup code here, to run once:

Serial.begin(9600);

}

void loop() {

// put your main code here, to run repeatedly:

int sensorvalue=analogRead(A0);//a0

Serial.println(sensorvalue);

}